|  |  |
| --- | --- |
|  | Job Safety Analysis |
| Portland State University  |  |
|  |  |  |
| Facilities Services |  |  |
| Operating a 24-inch Face Planer |
|  |
| **Task** | **Hazards** | **Controls** |
| 1. Start the exhaust fan.
 | Back draft of shavings  | Open exhaust vent. Wear safety glasses or face shield. |
| 2. Adjust table to desired thickness. | Jamming planer | Never plane more than 1/8 inch at a time. |
| 3. Start planer and place material into feeder. | Pinching fingers and hands | Avoid pinch points; release the material and allow feeder to pull it through the planer. |
| **Required Training:**1. Operation of face planer | **Required Personal Protective Equipment (PPE)**1. Safety glasses
2. Face shield
 |
|  |  |  |
| **Other Information:** |  |
| **Contributors:** | Reviewed JKM |
| **Created:** | July 2006 |