|  |  |  |  |
| --- | --- | --- | --- |
|  | Job Safety Analysis | | |
| Portland State University | |  |
|  |  |  |
| Facilities Services |  |  |
| Using a 6-Inch Notcher | | |
|  | | |
| **Task** | **Hazards** | **Controls** |
| 1. Align material and lower blade. | Lacerations to hand | Wear leather gloves.  Deburr test strips.  Do not slide hands along edges. |
| Pinching hand | Wear gloves.  Keep fingers from pinch point. |
| 2. Pull lever to shear metal. | Lacerations to hand | Wear leather gloves. |
| Pinching hand | Wear gloves.  Keep fingers from pinch point. |
| Muscle strain | Position body to support material, and get assistance when necessary. |
| 3. Remove metal from notcher. | Lacerations to hand | Wear leather gloves.  Do not slide hands along edges. |
| **Required Training:**   1. Learn capacity of equipment (maximum gauge of material) 2. Training in the operation of the notcher | **Required Personal Protective Equipment (PPE)**   1. Gloves 2. Non-slip shoes | |
|  |  |  |
| **Other Information:** |  | | |
| **Contributors:** | Reviewed JKM | | |
| **Created:** | July 2006 | | |